{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":162,"n_cols":10,"rows_kept":162,"cut":false,"hidden":false,"merged":[[161,0,161,11]]}
[]
[null,"FR450 - Tier 3"," FR480 - Stage V","FR500 - Tier 3"," FR550 - Stage V","FR650 - Tier 2"," FR650 - Stage V","FR780 - Tier 0"," FR780 - Stage V"," FR920 - Stage V"]
["Engine"]
["Engine ","FPT Cursor 13L*","FPT Cursor 13","FPT Cursor 13L*","FPT Cursor 13","FPT Cursor 16*","FPT Cursor 16","FPT Cursor 16L*","FPT Cursor 16","FPT V20"]
["Engine configuration and number of cylinders ","In-line 6","In-line 6","In-line 6","In-line 6","In-line 6","In-line 6","In-line 6","In-line 6","V8"]
["Capacity (cm³) ","12900","12900","12900","12900","15927","15927","15927","15927","20100"]
["Injection system ","Common Rail","Common Rail","Common Rail","Common Rail","Common Rail","Common Rail","Common Rail","Common Rail","Common Rail"]
["Compliant with engine emissions regulations"]
["Compliant with engine emissions regulations ","Tier 3 / Stage 3A","Stage V","Tier 3 / Stage 3A","Stage V","Tier 2","Stage V","Tier 0","Stage V","Stage V"]
["ECOBlue™ HI-eSCR 2 system (Selective Catalytic Reduction) ","-","Standard","-","Standard","-","Standard","-","Standard","Standard"]
["Gross engine power (2100rpm) - ISO TR14396 - ECE R119 [kW/hp(CV)] ","-","320/435","-","370/503","-","440/598","-","530/721","610/830"]
["Maximum engine power (1800-2000rpm) - ECE R120 [kW/hp(CV)] ","-","-","-","-","-","-","-","-","-"]
["Maximum engine power (1700-1900rpm) - ISO TR14396 - ECE R120 [kW/hp(CV)] ","331 / 450","350/476","366 / 498","400/544","480/653","480/653","570/775","570/775","670/911**"]
["Maximum Torque (1500rpm) ISO 14396 - ECE R120 (Nm)  ",null,"2003",null,"2316",null,"2751",null,"3323","4095"]
["Torque (1700rpm) ISO 14396 - ECE R120 (Nm)  ","-","1966","-","2247","-","2696","-","3202","3999***"]
["Torque (2100rpm to 1800rpm) ","-","-","-","-","-","-","-","-","-"]
["Torque rise (2100 to 1500rpm) (%) ","24%","38%","24","38%","37","37%","38","38%","48%"]
["Approved biodiesel blend**** ","-","B7","-","B7","-","B7","-","B7","B7"]
["Power Cruise™ II system ","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard"]
["ECO engine management mode ","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard"]
["Fuel consumption measuring and read-out on IntelliView™ IV monitor ","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard"]
["Radiator protection shield ","-","Optional","-","Optional","-","Optional","-","Optional","Optional"]
["Air compressor ","Optional","Optional","Optional","Optional","Optional","Optional","Standard","Optional","Standard"]
["Fuel tank"]
["Diesel capacity standard / optional (L) ","1200","1200 / 1500","1200","1200 / 1500","1200","1200 / 1500","1200","1200 / 1500","1200 / 1500"]
["AdBlue capacity (L) ","-","200","-","200","-","200","-","200","200"]
["Feeding"]
["Feeding ","HydroLoc™ drive","HydroLoc™ drive","HydroLoc™ drive","HydroLoc™ drive","HydroLoc™ drive","HydroLoc™ drive","HydroLoc™ drive","HydroLoc™ drive","HydroLoc™ drive"]
["RockAlert™ ","-","Optional","-","Optional","-","Optional","-","Optional","Optional"]
["Standard feedroll module ","-","Standard","-","Standard","-","Standard","-","Standard","-"]
["High performance feedroll module ","-","-","-","Optional","-","Optional","-","Optional","Standard"]
["Length of cut adjustment ","Infinite","Infinite","Infinite","Infinite","Infinite","Infinite","Infinite","Infinite","Infinite"]
["Number of feed-rolls (n°) ","4","4","4","4","4","4","4","4","4"]
["Feed opening width (mm) ","860 (33.86 inch)","860","860 (33.86 inch)","860","860 (33.86 inch)","860","860 (33.86 inch)","860","860"]
["MetaLoc™ metal detection with position indication ","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard"]
["Dual Drive system (header hydrostatic drive) ","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional"]
["ActiveLOC™ active chop length control ","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional"]
["Cutterhead"]
["Cutterhead cylinder type ","V--shaped with 2 rows of knives","V-shaped with 2 rows of knives","V-shaped with 2 rows of knives","V-shaped with 2 rows of knives","V-shaped with 2 rows of knives","V-shaped with 2 rows of knives","V-shaped with 2 rows of knives","V-shaped with 2 rows of knives"]
["Cutterhead frame width (mm) ","900","900","900","900","900","900","900","900","900"]
["Cutterhead cylinder width (mm) ","884","884","884","884","884","884","884","884","884"]
["Cutterhead diameter (max / min) (mm) ","710 / 690","710 / 690","710 / 690","710 / 690","710 / 690","710 / 690","710 / 690","710 / 690","710 / 690"]
["Cutterhead speed at 2100 engine rpm (rpm) ","1130","1130 / 1300 (2x20 knives)","1130","1130 / 1300 (2x20 knives)","1130","1130 / 1300 (2x20 knives)","1130","1130 / 1300 (2x20 knives)","1130 / 1300 (2x20 knives)"]
["Cuts per minute (2x8 knives) (c/min) ","9060","-","9060","-","9060","-","9060","-","-"]
["Length of cut range (2x8 knives) (mm) ","6 - 33","-","6 - 33","-","6 - 33","-","6 -33","-","-"]
["Cuts per minute (2x10 knives) (c/min) ","11320","11320","11320","11320","11320","11320","11320","11320","11320"]
["Length of cut range (2x10 knives) (mm) ","5-26","5/26/2024","5 - 26","5/26/2024","5 - 26","5/26/2024","5 -26","5/26/2024","5/26/2024"]
["Cuts per minute (2x12 knives) (c/min) ","13600","13600","13600","13600","13600","13600","13600","13600","13600"]
["Length of cut range (2x12 knives) (mm) ","4 - 22","4/22/2024","4 - 22","4/22/2024","4 - 22","4/22/2024","4 -22","4/22/2024","4/22/2024"]
["Cuts per minute (2x16 knives) (c/min) ","18100","18100","18100","18100","18100","18100","18100","18100","18100"]
["Length of cut range (2x16 knives) (mm) ","3 - 16","3/16/2024","3 - 16","3/16/2024","3 - 16","3/16/2024","3 - 16","3/16/2024","3/16/2024"]
["Cuts per minute (2x20 knives) (c/min) ","22600","-","22600","-","22600","22600","22600","22600","22600"]
["Length of cut range (2x20 knives) (mm) ","2 -13","-","2 - 13","-","2 - 13","2/13/2024","2 - 13","2/13/2024","2/13/2024"]
["Adjust-O-Matic™ shearbar setting ","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard"]
["Automatic knife sharpening system ","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard"]
["Automatic knife sharpening system with reverse drive ","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional"]
["Variflow™ system"]
["Variflow™ system ","Shift between crops in under two minutes","Shift between crops in under two minutes","Shift between crops in under two minutes","Shift between crops in under two minutes","Shift between crops in under two minutes","Shift between crops in under two minutes","Shift between crops in under two minutes","Shift between crops in under two minutes","Shift between crops in under two minutes"]
["Crop processor"]
["Standard Crop processor ","-","Standard","-","Standard","-","Standard","-","Standard","-"]
["Roll diameter (mm) ","200 / 250","250","250","250",null,"250","250","250","250"]
["Two-roll system with saw tooth profile (teeth) ","99 / 126 / 166","99 / 126 / 166","99 / 126 / 166","99 / 126 / 166",null,"99 / 126 / 166","99 / 126 / 166","99 / 126 / 166","-"]
["Chrome coated two-roll system with 99/126 Teeth combination ","-","-","-","Optional","-","Optional","-","Optional","-"]
["Width crop processor rolls (mm) ","750","750","750","750","750","750","750","750","750"]
["10% speed differential ","-","-","-","-","-","-","-","-","-"]
["22% speed differential ","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard","-"]
["30% speed differential always in combination with chrome coating ","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional","-"]
["50% speed differential (whole crop) ","-","-","-","-","-","-","-","-","-"]
["60% speed differential (whole crop) ","-","Optional","-","Optional","-","Optional","-","Optional","-"]
["Roll clearance range (electro-hydraulic adjustment) (mm) ","1-6","1/6/2024","1-6","1/6/2024","1-6","1/6/2024","1-6","1/6/2024","-"]
["Manual clearance control (optional 200mm rolls) ","Optional","Optional","Optional","-","-","-","-","-","-"]
["Remote electro-hydraulic clearance control (250mm rolls) ","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard","-"]
["DuraCracker™ Heavy Duty Crop processor"]
["DuraCracker™ Heavy Duty Crop processor ","-","Optional","-","Optional","-","Optional","-","Optional","Standard"]
["Roll diameter (mm) ","-","250","-","250","-","250","-","250","250"]
["Two chrome roll system with DuraCracker™ saw tooth profile (teeth) ","-","100 / 130","-","100 / 130","-","100 / 130","-","100 / 130","100 / 130"]
["Two chrome roll system with DuraShredder™ spiral cut tooth profile (teeth) ","-","110 / 145","-","110 / 145","-","110 / 145","-","110 / 145","110 / 145"]
["Width crop processor rolls (mm) ","-","750","-","750","-","750","-","750","750"]
["30% speed differential ","-","Standard","-","Standard","-","Standard","-","Standard","Standard"]
["40% speed differential ","-","Optional","-","Optional","-","Optional","-","Optional","Optional"]
["Roll clearance range (electro-hydraulic adjustment) (mm) ","-","1/4/2024","-","1/4/2024","-","1/4/2024","-","1/4/2024","1/4/2024"]
["Remote electro-hydraulic clearance control ","-","Standard","-","Standard","-","Standard","-","Standard","Standard"]
["Blower"]
["Blower rotor diameter (mm) ","525","525","525","525","525","525","525","525","525"]
["Blower rotor width (mm) ","750","750","750","750","750","750","750","750","750"]
["Blower speed at 2100 engine rpm (rpm) ","2119","2119","2119","2119","2119","2119","2119","2119","2119"]
["Spout"]
["Spout maximum height (mm) ","6400","6400","6400","6400","6400","6400","6400","6400","6400"]
["Rotation angle (°) ","210","210","210","210","210","210","210","210","210"]
["Spout extension (10-row maize header) (mm) ","720","720","720","720","720","720","720","720","720"]
["Spout extension (12-row maize header) (mm) ","1380","1380","1380","1380","1380","1380","1380","1380","1380"]
["Automatic spout functions (home and work positions) ","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard"]
["Spout side collision protection ","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard"]
["Abrasive option"]
["Abrasive options ","-","Optional","-","Optional","-","Optional","-","Optional","Optional"]
["Spout ","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional"]
["Cropflow ","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional"]
["Electrical"]
["12 volt alternator Standard / Optional (Amps) ","240","240","240","240","240","240","240","240","240"]
["Battery capacity (CCA / Ah) ","2 x 800 /107","2x800 / 107","2 x 800 /107","2x800 / 107","3 x 800 /107","3x800 / 107","3 x 800 /107","3x800 / 107","4x800 / 107"]
["Transmission"]
["Hydrostatic ","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard"]
["Gearbox ","4-speed","4-speed","4-speed","4-speed","4-speed","4-speed","4-Speed","4-speed","4-speed"]
["Remote gearshifting ","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard"]
["Differential lock ","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional"]
["Mechanical powered rear wheels ","-","-","-","-","-","-","-","-","-"]
["Mechanical 4WD system ","-","Optional","-","Optional","-","Optional","-","Optional","-"]
["Heavy duty 4WD system with Terralock™ traction management ","-","Optional",null,"Optional","-","Optional","-","Optional","Optional"]
["Maximum optional road speed @ 1200rpm (kph) ","40","40","40","40","40","40","40","40","40"]
["Header control systems"]
["Automatic stubble height control ","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard"]
["Pressure compensation mode ","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard"]
["Autofloat™ system ","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional"]
["Mechanical Lateral flotation ","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard"]
["Power Reverse hydraulic header reverser ","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard"]
["Hydraulic quick coupler (single location) ","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard"]
["Automatic header speed synchronisation to forward speed ","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard"]
["Cab glass area"]
["Cab glass area (m³) ","6.8","6/8/2024","6.8","6/8/2024","6.8","6/8/2024","6.8","6/8/2024","6/8/2024"]
["Cab category level - EN 15695 ","1","1","1",null,"1","1","1","1"]
["LED lighting pack ","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional"]
["Standard cloth trimmed seat with air-suspension ","Standard","Standard","Standard","Standard","Standard","6/8/2024","Standard","Standard","Standard"]
["Deluxe cloth trimmed heated air-suspension seat with Active Ventilation ","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional"]
["Leather trimmed heated air-suspension seat with Active Ventilation ","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional"]
["Instructor’s seat ","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard"]
["CommandGrip™ handle ","Optional","Standard","Optional","Standard","Optional","Standard","Optional","Standard","Standard"]
["IntelliView™ IV monitor with adjustable position ","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard"]
["2nd IntelliView™ IV monitor ","-","Optional","-","Optional","-","Optional","-","Optional","Optional"]
["ISOBUS (Virtual Terminal) compatibility ","-","Optional","-","Optional","-","Optional","-","Optional","Optional"]
["Air horn [dual-trumpet, 150/180Hz, 112dB(A)] ","-","Optional","-","Optional","-","Optional","-","Optional","Optional"]
["Accessory mounting rail ","-","Optional","-","Optional","-","Optional","-","Optional","Optional"]
["Reversing camera ","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional"]
["Manual air-conditioning and heating ","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard"]
["Automatic climate control ","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional"]
["Removable coolbox ","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional"]
["MP3 Bluetooth radio (hands free phone calls) ","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional"]
["2 x USB charging ports ","-","Standard","-","Standard","-","Standard","-","Standard","Standard"]
["Automatic greasing system ","Optional","Standard","Optional","Standard","Optional","Standard","Optional","Standard","Standard"]
["Rear bumper with integrated water proof storage boxes ","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard"]
["Optimum cab noise level - ISO 5131 (dB(A)) ","76","76","76","76","76","76","76","76","76"]
["New Holland Intelligence Systems - New Holland FieldOps™ Telematics"]
["New Holland FieldOps™ Telematics Professional (3 year subscription free)  ","Optional","Standard","Optional","Standard","Optional","Standard","Optional","Standard","Standard"]
["New Holland FieldOps™ Telematics Professional (3 or 5 year subscription)  ","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional"]
["New Holland Intelligence Systems - Guidance systems"]
["IntelliSteer® ready automatic guidance system ","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional"]
["Automatic row guidance system for maize headers ","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional"]
["IntelliFill™ system (automated side and rear trailer filling) ","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional"]
["New Holland Intelligence Systems - Precision farming"]
["Optional additive tank (with adjustable flow) capacity (L) ","395","Optional","395","Optional","395","Optional","395","Optional","Optional"]
["Moisture measuring ","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional"]
["Yield measuring and moisture measuring ","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional"]
["Full Precision farming package including: Yield measuring and moisture measuring, DGPS yield mapping ","-","-","-","Optional","Optional","Optional","-","-","Optional"]
["Full Precision farming package including: PLM® desktop software and software support service ","-","-","-","Optional","Optional","Optional","-","-","Optional"]
["NutriSense™ NIR sensor nutrient analysis technology  ","-","Optional","-","Optional","-","Optional","-","Optional","Optional"]
["New Holland FieldOps™ Farm tab agronomic data visualisation - USB  ","-","Standard","-","Standard","-","Standard","-","Standard","Standard"]
["New Holland FieldOps™ Farm tab file transfer – Professional (3 years subscription)  ","-","Optional","-","Optional","-","Optional","-","Optional","Optional"]
["Uptime Solutions - Training & Support Systems"]
["New Holland Proactive Breakdown Support  ","-","Optional","-","Optional","-","Optional","-","Optional","Optional"]
["New Holland Breakdown Assist  ","-","Optional","-","Optional","-","Optional","-","Optional","Optional"]
["Weight****"]
["Weight**** (kg) ","12250","13050","12750","13100","12760","13550","13060","13650","15540"]
["​* Developed by FPT Industrial       \n** Engine speed 1800 - 2000rpm       \n*** Engine speed at 1800rpm       \n**** Biodiesel blend must fully comply with the latest fuel specification EN14214:2009 and operation is in accordance with operator manual guidelines       \n***** Minimum empty weight for basic grass configuration"]